| Mozzi version v1.1.0 sound synthesis library for Arduino |

02.Control/Control_Echo_Theremin/Control_Echo_Theremin.ino

This is an example of how to use the ControlDelay class.

/* Example of a simple light-sensing theremin-like
instrument with long echoes,
using Mozzi sonification library.
Demonstrates ControlDelay() for echoing control values,
and smoothing an analog input from a sensor
signal with RollingAverage().
The circuit:
Audio output on digital pin 9 on a Uno or similar, or
DAC/A14 on Teensy 3.1, or
check the README or http://sensorium.github.io/Mozzi/
Light dependent resistor (LDR) and 5.1k resistor on analog pin 1:
LDR from analog pin to +5V (3.3V on Teensy 3.1)
5.1k resistor from analog pin to ground
Mozzi documentation/API
https://sensorium.github.io/Mozzi/doc/html/index.html
Mozzi help/discussion/announcements:
https://groups.google.com/forum/#!forum/mozzi-users
Tim Barrass 2013, CC by-nc-sa.
*/
#include <MozziGuts.h>
#include <Oscil.h> // oscillator template
#include <tables/sin2048_int8.h> // sine table for oscillator
#include <RollingAverage.h>
#include <ControlDelay.h>
#define INPUT_PIN 0 // analog control input
#define CONTROL_RATE 64
unsigned int echo_cells_1 = 32;
unsigned int echo_cells_2 = 60;
unsigned int echo_cells_3 = 127;
ControlDelay <128, int> kDelay; // 2seconds
// oscils to compare bumpy to averaged control input
Oscil <SIN2048_NUM_CELLS, AUDIO_RATE> aSin0(SIN2048_DATA);
Oscil <SIN2048_NUM_CELLS, AUDIO_RATE> aSin1(SIN2048_DATA);
Oscil <SIN2048_NUM_CELLS, AUDIO_RATE> aSin2(SIN2048_DATA);
Oscil <SIN2048_NUM_CELLS, AUDIO_RATE> aSin3(SIN2048_DATA);
// use: RollingAverage <number_type, how_many_to_average> myThing
RollingAverage <int, 32> kAverage; // how_many_to_average has to be power of 2
int averaged;
void setup(){
kDelay.set(echo_cells_1);
startMozzi();
}
void updateControl(){
int bumpy_input = mozziAnalogRead(INPUT_PIN);
averaged = kAverage.next(bumpy_input);
aSin0.setFreq(averaged);
aSin1.setFreq(kDelay.next(averaged));
aSin2.setFreq(kDelay.read(echo_cells_2));
aSin3.setFreq(kDelay.read(echo_cells_3));
}
AudioOutput_t updateAudio(){
return MonoOutput::almostNBit(12,
3*((int)aSin0.next()+aSin1.next()+(aSin2.next()>>1)
+(aSin3.next()>>2))
);
);
}
void loop(){
audioHook();
}