| Mozzi version v1.1.0 sound synthesis library for Arduino |

05.Control_Filters/DCFilter/DCFilter.ino

This example demonstrates the DCFilter class.

/* Example of filtering an analog input to remove DC bias,
using Mozzi sonification library.
Demonstrates DCfilter(), DC-blocking filter useful for
highlighting changes in control signals.
The output of the filter settles to 0 if the incoming signal stays constant.
If the input changes, the filter output swings to track the change and
eventually settles back to 0.
Mozzi documentation/API
https://sensorium.github.io/Mozzi/doc/html/index.html
Mozzi help/discussion/announcements:
https://groups.google.com/forum/#!forum/mozzi-users
Tim Barrass 2013, CC by-nc-sa.
*/
#include <MozziGuts.h>
#include <DCfilter.h>
int sensorPin = A0;
DCfilter dcFiltered(0.9); // parameter sets how long the filter takes to settle
void setup() {
//Serial.begin(9600); // for Teensy 3.1, beware printout can cause glitches
Serial.begin(115200);
startMozzi();
}
void updateControl(){
// read the value from the sensor:
int sensorValue = mozziAnalogRead(sensorPin);
Serial.print(sensorValue);
Serial.print(" Filtered = ");
Serial.println(dcFiltered.next(sensorValue));
}
AudioOutput_t updateAudio(){
return 0;
}
void loop(){
audioHook();
}