| Mozzi version v1.1.0 sound synthesis library for Arduino |

Here is a list of all documented class members with links to the class documentation for each member:

### - s -

- Sample() : Sample< NUM_TABLE_CELLS, UPDATE_RATE, INTERP >
- SampleHuffman() : SampleHuffman
- set() : AudioDelay< NUM_BUFFER_SAMPLES, T > , Ead , EventDelay , Line< T > , Line< unsigned char > , Line< unsigned int > , Line< unsigned long > , Phasor< UPDATE_RATE > , WavePacket< ALGORITHM >
- setADLevels() : ADSR< CONTROL_UPDATE_RATE, LERP_RATE, T >
- setAllUpdateSteps() : ADSR< CONTROL_UPDATE_RATE, LERP_RATE, T > , MultiLine< CONTROL_UPDATE_RATE, LERP_RATE >
- setAttack() : Ead
- setAttackLevel() : ADSR< CONTROL_UPDATE_RATE, LERP_RATE, T >
- setAttackTime() : ADSR< CONTROL_UPDATE_RATE, LERP_RATE, T >
- setAttackUpdateSteps() : ADSR< CONTROL_UPDATE_RATE, LERP_RATE, T >
- setBandwidth() : WavePacket< ALGORITHM >
- setBPM() : Metronome
- setCentreFreq() : StateVariable< FILTER_TYPE > , WavePacket< ALGORITHM >
- setCutoffFreq() : LowPassFilter
- setCutoffFreqAndResonance() : LowPassFilter
- setDecay() : Ead
- setDecayLevel() : ADSR< CONTROL_UPDATE_RATE, LERP_RATE, T >
- setDecayTime() : ADSR< CONTROL_UPDATE_RATE, LERP_RATE, T >
- setDecayUpdateSteps() : ADSR< CONTROL_UPDATE_RATE, LERP_RATE, T >
- setDelayTimeCells() : AudioDelayFeedback< NUM_BUFFER_SAMPLES, INTERP_TYPE >
- setEarlyReflections() : ReverbTank
- setEnd() : Sample< NUM_TABLE_CELLS, UPDATE_RATE, INTERP >
- setFeebackLevel() : ReverbTank
- setFeedbackLevel() : AudioDelayFeedback< NUM_BUFFER_SAMPLES, INTERP_TYPE >
- setFreq() : Oscil< NUM_TABLE_CELLS, UPDATE_RATE > , Phasor< UPDATE_RATE > , Sample< NUM_TABLE_CELLS, UPDATE_RATE, INTERP >
- setFreq_Q16n16() : Oscil< NUM_TABLE_CELLS, UPDATE_RATE >
- setFreq_Q24n8() : Oscil< NUM_TABLE_CELLS, UPDATE_RATE > , Sample< NUM_TABLE_CELLS, UPDATE_RATE, INTERP >
- setFundamental() : WavePacket< ALGORITHM >
- setLevels() : ADSR< CONTROL_UPDATE_RATE, LERP_RATE, T > , MultiLine< CONTROL_UPDATE_RATE, LERP_RATE >
- setLoopDelays() : ReverbTank
- setLoopingOff() : Sample< NUM_TABLE_CELLS, UPDATE_RATE, INTERP > , SampleHuffman
- setLoopingOn() : Sample< NUM_TABLE_CELLS, UPDATE_RATE, INTERP > , SampleHuffman
- setPDEnv() : PDResonant
- setPhase() : Oscil< NUM_TABLE_CELLS, UPDATE_RATE >
- setPhaseFractional() : Oscil< NUM_TABLE_CELLS, UPDATE_RATE >
- setPhaseInc() : Oscil< NUM_TABLE_CELLS, UPDATE_RATE > , Phasor< UPDATE_RATE > , Sample< NUM_TABLE_CELLS, UPDATE_RATE, INTERP >
- setReleaseLevel() : ADSR< CONTROL_UPDATE_RATE, LERP_RATE, T >
- setReleaseTime() : ADSR< CONTROL_UPDATE_RATE, LERP_RATE, T >
- setReleaseUpdateSteps() : ADSR< CONTROL_UPDATE_RATE, LERP_RATE, T >
- setResonance() : LowPassFilter , StateVariable< FILTER_TYPE >
- setSmoothness() : Smooth< T >
- setStart() : Sample< NUM_TABLE_CELLS, UPDATE_RATE, INTERP >
- setSustainLevel() : ADSR< CONTROL_UPDATE_RATE, LERP_RATE, T >
- setSustainTime() : ADSR< CONTROL_UPDATE_RATE, LERP_RATE, T >
- setSustainUpdateSteps() : ADSR< CONTROL_UPDATE_RATE, LERP_RATE, T >
- setTable() : Oscil< NUM_TABLE_CELLS, UPDATE_RATE > , Sample< NUM_TABLE_CELLS, UPDATE_RATE, INTERP > , WavePacketSample< ALGORITHM >
- setTarget1Level() : MultiLine< CONTROL_UPDATE_RATE, LERP_RATE >
- setTarget1Time() : MultiLine< CONTROL_UPDATE_RATE, LERP_RATE >
- setTarget1UpdateSteps() : MultiLine< CONTROL_UPDATE_RATE, LERP_RATE >
- setTarget2Level() : MultiLine< CONTROL_UPDATE_RATE, LERP_RATE >
- setTarget2Time() : MultiLine< CONTROL_UPDATE_RATE, LERP_RATE >
- setTarget2UpdateSteps() : MultiLine< CONTROL_UPDATE_RATE, LERP_RATE >
- setTarget3Level() : MultiLine< CONTROL_UPDATE_RATE, LERP_RATE >
- setTarget3Time() : MultiLine< CONTROL_UPDATE_RATE, LERP_RATE >
- setTarget3UpdateSteps() : MultiLine< CONTROL_UPDATE_RATE, LERP_RATE >
- setTarget4Level() : MultiLine< CONTROL_UPDATE_RATE, LERP_RATE >
- setTarget4Time() : MultiLine< CONTROL_UPDATE_RATE, LERP_RATE >
- setTarget4UpdateSteps() : MultiLine< CONTROL_UPDATE_RATE, LERP_RATE >
- setTargetLevel() : MultiLine< CONTROL_UPDATE_RATE, LERP_RATE >
- setTargetTime() : MultiLine< CONTROL_UPDATE_RATE, LERP_RATE >
- setTargetUpdateSteps() : MultiLine< CONTROL_UPDATE_RATE, LERP_RATE >
- setTime() : Portamento< CONTROL_UPDATE_RATE >
- setTimes() : ADSR< CONTROL_UPDATE_RATE, LERP_RATE, T > , MultiLine< CONTROL_UPDATE_RATE, LERP_RATE >
- Smooth() : Smooth< T >
- Stack() : Stack< T, NUM_ITEMS >
- start() : Ead , EventDelay , Metronome , MultiLine< CONTROL_UPDATE_RATE, LERP_RATE > , Portamento< CONTROL_UPDATE_RATE > , Sample< NUM_TABLE_CELLS, UPDATE_RATE, INTERP > , SampleHuffman
- StateVariable() : StateVariable< FILTER_TYPE >
- StereoOutput() : StereoOutput
- stop() : MultiLine< CONTROL_UPDATE_RATE, LERP_RATE >