A C D G H I L M O P S U V W

## A

Arm - Class in de.voidplus.myo
Arm.Type - Enum in de.voidplus.myo

## C

Collector - Class in de.voidplus.myo
Collector(Myo) - Constructor for class de.voidplus.myo.Collector

## D

de.voidplus.myo - package de.voidplus.myo
dispose() - Method in class de.voidplus.myo.Myo

## G

getAccelerometer() - Method in class de.voidplus.myo.Myo
  Get gyroscope values of device.
getArm() - Method in class de.voidplus.myo.Myo
  Get the type of recognized arm.
getEmg() - Method in class de.voidplus.myo.Myo
  Get raw data of EMG sensors.
getFirmware() - Method in class de.voidplus.myo.Myo
  Get the firmware of device.
getGyroscope() - Method in class de.voidplus.myo.Myo
  Get gyroscope values of device.
getOrientation() - Method in class de.voidplus.myo.Myo
  Get orientation values of device.
getPose() - Method in class de.voidplus.myo.Myo
  Get the name of the latest pose.
getRawHub() - Method in class de.voidplus.myo.Myo
  Get access to the raw instance of class Hub.
getRawMyo() - Method in class de.voidplus.myo.Myo
  Get access to the raw instance of class Myo.
getType() - Method in class de.voidplus.myo.Arm
  Get the type of arm.
getType() - Method in class de.voidplus.myo.Pose
  Get the type of pose.

## H

hasArm() - Method in class de.voidplus.myo.Myo
  Arm recognized?

## I

isArmLeft() - Method in class de.voidplus.myo.Myo
  Left arm?
isArmRight() - Method in class de.voidplus.myo.Myo
  Right arm?
isLeft() - Method in class de.voidplus.myo.Arm
  Left arm?
isRight() - Method in class de.voidplus.myo.Arm
  Right arm? For humans with more than two arms.

## L

lock() - Method in class de.voidplus.myo.Myo
  Force the Myo to lock immediately.

## M

Myo - Class in de.voidplus.myo
Myo(PApplet) - Constructor for class de.voidplus.myo.Myo
Myo.Event - Enum in de.voidplus.myo
Myo.LockingPolicy - Enum in de.voidplus.myo
Myo.Unlock - Enum in de.voidplus.myo

## O

onAccelerometerData(Myo, long, Vector3) - Method in class de.voidplus.myo.Collector
onArmSync(Myo, long, Arm, XDirection) - Method in class de.voidplus.myo.Collector
onArmUnsync(Myo, long) - Method in class de.voidplus.myo.Collector
onConnect(Myo, long, FirmwareVersion) - Method in class de.voidplus.myo.Collector
onDisconnect(Myo, long) - Method in class de.voidplus.myo.Collector
onEmgData(Myo, long, byte[]) - Method in class de.voidplus.myo.Collector
onGyroscopeData(Myo, long, Vector3) - Method in class de.voidplus.myo.Collector
onLock(Myo, long) - Method in class de.voidplus.myo.Collector
onOrientationData(Myo, long, Quaternion) - Method in class de.voidplus.myo.Collector
onPair(Myo, long, FirmwareVersion) - Method in class de.voidplus.myo.Collector
onPose(Myo, long, com.thalmic.myo.Pose) - Method in class de.voidplus.myo.Collector
onRssi(Myo, long, int) - Method in class de.voidplus.myo.Collector
onUnlock(Myo, long) - Method in class de.voidplus.myo.Collector
onUnpair(Myo, long) - Method in class de.voidplus.myo.Collector

## P

Pose - Class in de.voidplus.myo
Pose.Type - Enum in de.voidplus.myo
pre() - Method in class de.voidplus.myo.Myo

## S

setFrequency(int) - Method in class de.voidplus.myo.Myo
  Set the duration to access data.
setLockingPolicy(Myo.LockingPolicy) - Method in class de.voidplus.myo.Myo
  Set the locking policy for Myos connected to the Hub.
setVerbose(boolean) - Method in class de.voidplus.myo.Myo
  Print debug information to the console.
setVerboseLevel(int) - Method in class de.voidplus.myo.Myo
  Set the level of the log level.

## U

unlock(Myo.Unlock) - Method in class de.voidplus.myo.Myo
  Unlock the Myo.

## V

valueOf(String) - Static method in enum de.voidplus.myo.Arm.Type
  Returns the enum constant of this type with the specified name.
valueOf(String) - Static method in enum de.voidplus.myo.Myo.Event
  Returns the enum constant of this type with the specified name.
valueOf(String) - Static method in enum de.voidplus.myo.Myo.LockingPolicy
  Returns the enum constant of this type with the specified name.
valueOf(String) - Static method in enum de.voidplus.myo.Myo.Unlock
  Returns the enum constant of this type with the specified name.
valueOf(String) - Static method in enum de.voidplus.myo.Pose.Type
  Returns the enum constant of this type with the specified name.
values() - Static method in enum de.voidplus.myo.Arm.Type
  Returns an array containing the constants of this enum type, in the order they are declared.
values() - Static method in enum de.voidplus.myo.Myo.Event
  Returns an array containing the constants of this enum type, in the order they are declared.
values() - Static method in enum de.voidplus.myo.Myo.LockingPolicy
  Returns an array containing the constants of this enum type, in the order they are declared.
values() - Static method in enum de.voidplus.myo.Myo.Unlock
  Returns an array containing the constants of this enum type, in the order they are declared.
values() - Static method in enum de.voidplus.myo.Pose.Type
  Returns an array containing the constants of this enum type, in the order they are declared.
vibrate(int) - Method in class de.voidplus.myo.Myo
  The device will vibrate for haptic feedback.
vibrate() - Method in class de.voidplus.myo.Myo

## W

withEmg() - Method in class de.voidplus.myo.Myo
  Enable EMG mode.
withoutEmg() - Method in class de.voidplus.myo.Myo
  Disable EMG mode.

A C D G H I L M O P S U V W

Processing library MyoForProcessing by Darius Morawiec. (C) 2014