## Muse Developer Resources | Search this site

MuseIO‎ > ‎ ### Available Data Modes (Presets)
## Muse can be configured by MuseIO in different ways by specifying “--preset <PRESET>” as an option on the command line. The following presets are available: SPS = samples per second
| Preset ID | EEG Channels | EEG Data | Accelerometer Data | Notch Filter | Compression | Battery/Temp Data | Error Data | DRL/REF Data
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
Consumer Presets | 10 | TP9, Fp1, Fp2, TP10 | 10 bits @ 220Hz | None | 60Hz | ON | None | None | None
12 | TP9, Fp1, Fp2, TP10 | 10 bits @ 220Hz | 50Hz | 60Hz | ON | 0.1Hz | None | None
14 | TP9, Fp1, Fp2, TP10 | 10 bits @ 220Hz | 50Hz | 60Hz | ON | 0.1Hz | Real-time | 10bit @ 10Hz
Research Presets | AD | TP9, Fp1, Fp2, TP10 | 16 bits @ 500Hz | 50Hz | OFF | OFF | 0.1Hz | None | None
AE | TP9, Fp1, Fp2, TP10, DRL, REF | 16 bits @ 500Hz | 50Hz | OFF | OFF | 0.1Hz | Real-time | Included in EEG packet
Comments