| Mozzi version v1.1.0 sound synthesis library for Arduino |

MultiLine< CONTROL_UPDATE_RATE, LERP_RATE > Member List

This is the complete list of members for MultiLine< CONTROL_UPDATE_RATE, LERP_RATE >, including all inherited members.

MultiLine() | MultiLine< CONTROL_UPDATE_RATE, LERP_RATE > | inline
MultiLine() | MultiLine< CONTROL_UPDATE_RATE, LERP_RATE > | inline
next() | MultiLine< CONTROL_UPDATE_RATE, LERP_RATE > | inline
next() | MultiLine< CONTROL_UPDATE_RATE, LERP_RATE > | inline
playing() | MultiLine< CONTROL_UPDATE_RATE, LERP_RATE > | inline
playing() | MultiLine< CONTROL_UPDATE_RATE, LERP_RATE > | inline
setAllUpdateSteps(unsigned int target1_steps, unsigned int target2_steps, unsigned int target3_steps, unsigned int target4_steps) | MultiLine< CONTROL_UPDATE_RATE, LERP_RATE > | inline
setIdleLevel(Q15n16 value) (defined in MultiLine< CONTROL_UPDATE_RATE, LERP_RATE >) | MultiLine< CONTROL_UPDATE_RATE, LERP_RATE > | inline
setIdleTime(unsigned int msec) (defined in MultiLine< CONTROL_UPDATE_RATE, LERP_RATE >) | MultiLine< CONTROL_UPDATE_RATE, LERP_RATE > | inline
setIdleUpdateSteps(unsigned int steps) (defined in MultiLine< CONTROL_UPDATE_RATE, LERP_RATE >) | MultiLine< CONTROL_UPDATE_RATE, LERP_RATE > | inline
setLevels(Q15n16 target1, Q15n16 target2, Q15n16 target3, Q15n16 target4) | MultiLine< CONTROL_UPDATE_RATE, LERP_RATE > | inline
setTarget1Level(Q15n16 value) | MultiLine< CONTROL_UPDATE_RATE, LERP_RATE > | inline
setTarget1Time(unsigned int msec) | MultiLine< CONTROL_UPDATE_RATE, LERP_RATE > | inline
setTarget1UpdateSteps(unsigned int steps) | MultiLine< CONTROL_UPDATE_RATE, LERP_RATE > | inline
setTarget2Level(Q15n16 value) | MultiLine< CONTROL_UPDATE_RATE, LERP_RATE > | inline
setTarget2Time(unsigned int msec) | MultiLine< CONTROL_UPDATE_RATE, LERP_RATE > | inline
setTarget2UpdateSteps(unsigned int steps) | MultiLine< CONTROL_UPDATE_RATE, LERP_RATE > | inline
setTarget3Level(Q15n16 value) | MultiLine< CONTROL_UPDATE_RATE, LERP_RATE > | inline
setTarget3Time(unsigned int msec) | MultiLine< CONTROL_UPDATE_RATE, LERP_RATE > | inline
setTarget3UpdateSteps(unsigned int steps) | MultiLine< CONTROL_UPDATE_RATE, LERP_RATE > | inline
setTarget4Level(Q15n16 value) | MultiLine< CONTROL_UPDATE_RATE, LERP_RATE > | inline
setTarget4Time(unsigned int msec) | MultiLine< CONTROL_UPDATE_RATE, LERP_RATE > | inline
setTarget4UpdateSteps(unsigned int steps) | MultiLine< CONTROL_UPDATE_RATE, LERP_RATE > | inline
setTargetLevel(uint8_t phase_num, Q15n16 value) | MultiLine< CONTROL_UPDATE_RATE, LERP_RATE > | inline
setTargetTime(uint8_t phase_num, unsigned int msec) | MultiLine< CONTROL_UPDATE_RATE, LERP_RATE > | inline
setTargetUpdateSteps(uint8_t phase_num, unsigned int steps) | MultiLine< CONTROL_UPDATE_RATE, LERP_RATE > | inline
setTimes(unsigned int target1_ms, unsigned int target2_ms, unsigned int target3_ms, unsigned int target4_ms) | MultiLine< CONTROL_UPDATE_RATE, LERP_RATE > | inline
start() | MultiLine< CONTROL_UPDATE_RATE, LERP_RATE > | inline
start() | MultiLine< CONTROL_UPDATE_RATE, LERP_RATE > | inline
stop() | MultiLine< CONTROL_UPDATE_RATE, LERP_RATE > | inline
stop() | MultiLine< CONTROL_UPDATE_RATE, LERP_RATE > | inline
update() | MultiLine< CONTROL_UPDATE_RATE, LERP_RATE > | inline
update() | MultiLine< CONTROL_UPDATE_RATE, LERP_RATE > | inline