| Mozzi version v1.1.0 sound synthesis library for Arduino |

ADSR< CONTROL_UPDATE_RATE, LERP_RATE, T > Member List

This is the complete list of members for ADSR< CONTROL_UPDATE_RATE, LERP_RATE, T >, including all inherited members.

ADSR() | ADSR< CONTROL_UPDATE_RATE, LERP_RATE, T > | inline
adsr_playing (defined in ADSR< CONTROL_UPDATE_RATE, LERP_RATE, T >) | ADSR< CONTROL_UPDATE_RATE, LERP_RATE, T > |
next() | ADSR< CONTROL_UPDATE_RATE, LERP_RATE, T > | inline
noteOff() | ADSR< CONTROL_UPDATE_RATE, LERP_RATE, T > | inline
noteOn(bool reset=false) | ADSR< CONTROL_UPDATE_RATE, LERP_RATE, T > | inline
playing() | ADSR< CONTROL_UPDATE_RATE, LERP_RATE, T > | inline
setADLevels(byte attack, byte decay) | ADSR< CONTROL_UPDATE_RATE, LERP_RATE, T > | inline
setAllUpdateSteps(unsigned int attack_steps, unsigned int decay_steps, unsigned int sustain_steps, unsigned int release_steps) | ADSR< CONTROL_UPDATE_RATE, LERP_RATE, T > | inline
setAttackLevel(byte value) | ADSR< CONTROL_UPDATE_RATE, LERP_RATE, T > | inline
setAttackTime(unsigned int msec) | ADSR< CONTROL_UPDATE_RATE, LERP_RATE, T > | inline
setAttackUpdateSteps(unsigned int steps) | ADSR< CONTROL_UPDATE_RATE, LERP_RATE, T > | inline
setDecayLevel(byte value) | ADSR< CONTROL_UPDATE_RATE, LERP_RATE, T > | inline
setDecayTime(unsigned int msec) | ADSR< CONTROL_UPDATE_RATE, LERP_RATE, T > | inline
setDecayUpdateSteps(unsigned int steps) | ADSR< CONTROL_UPDATE_RATE, LERP_RATE, T > | inline
setIdleLevel(byte value) (defined in ADSR< CONTROL_UPDATE_RATE, LERP_RATE, T >) | ADSR< CONTROL_UPDATE_RATE, LERP_RATE, T > | inline
setIdleTime(unsigned int msec) (defined in ADSR< CONTROL_UPDATE_RATE, LERP_RATE, T >) | ADSR< CONTROL_UPDATE_RATE, LERP_RATE, T > | inline
setIdleUpdateSteps(unsigned int steps) (defined in ADSR< CONTROL_UPDATE_RATE, LERP_RATE, T >) | ADSR< CONTROL_UPDATE_RATE, LERP_RATE, T > | inline
setLevels(byte attack, byte decay, byte sustain, byte release) | ADSR< CONTROL_UPDATE_RATE, LERP_RATE, T > | inline
setReleaseLevel(byte value) | ADSR< CONTROL_UPDATE_RATE, LERP_RATE, T > | inline
setReleaseTime(unsigned int msec) | ADSR< CONTROL_UPDATE_RATE, LERP_RATE, T > | inline
setReleaseUpdateSteps(unsigned int steps) | ADSR< CONTROL_UPDATE_RATE, LERP_RATE, T > | inline
setSustainLevel(byte value) | ADSR< CONTROL_UPDATE_RATE, LERP_RATE, T > | inline
setSustainTime(unsigned int msec) | ADSR< CONTROL_UPDATE_RATE, LERP_RATE, T > | inline
setSustainUpdateSteps(unsigned int steps) | ADSR< CONTROL_UPDATE_RATE, LERP_RATE, T > | inline
setTimes(unsigned int attack_ms, unsigned int decay_ms, unsigned int sustain_ms, unsigned int release_ms) | ADSR< CONTROL_UPDATE_RATE, LERP_RATE, T > | inline
update() | ADSR< CONTROL_UPDATE_RATE, LERP_RATE, T > | inline