| Mozzi version v1.1.0 sound synthesis library for Arduino |

Class List
Here are the classes, structs, unions and interfaces with brief descriptions:

C ADSR | A simple ADSR envelope generator
C AudioDelay | Audio delay line for comb filter, flange, chorus and short echo effects
C AudioDelayFeedback | Audio delay line with feedback for comb filter, flange, chorus and short echo effects
C AutoMap | Automatically map an input value to an output range without knowing the precise range of inputs beforehand
C AutoRange | Keeps a running calculation of the range of the input values it receives
C CapPoll | A class for reading voltage on a digital pin, derived from http://arduino.cc/en/Tutorial/RCtime
C CircularBuffer | Circular buffer object
C ControlDelay | Control-rate delay line for delaying control signals
C DCfilter | A DC-blocking filter useful for highlighting changes in control signals
C Ead | Exponential attack decay envelope
C EventDelay | A non-blocking replacement for Arduino's delay() function
C Int2Type | Enables you to instantiate a template based on an integer value
C IntMap | A faster version of Arduino's map() function
C Line | For linear changes with a minimum of calculation at each step
C Line< unsigned char > |
C Line< unsigned int > |
C Line< unsigned long > |
C LowPassFilter | A resonant low pass filter for audio signals
C Metronome | A metronome class which is like an EventDelay which retriggers itself when the delay time is up, to produce a repeating beat
C MonoOutput | This struct encapsulates one frame of mono audio output
C MultiLine | A simple MultiLine envelope generator
C Oscil | Oscil plays a wavetable, cycling through the table to generate an audio or control signal
C OverSample | Enables the resolution of analog inputs to be increased by oversampling and decimation
C PDResonant | PDResonant is a simple midi instrument using Phase distortion used to simulate resonant filter, based on https://en.wikipedia.org/wiki/Phase_distortion_synthesis
C Phasor | Phasor repeatedly generates a high resolution ramp at a variable frequency
C Portamento | A simple portamento (pitch slide from one note to the next) effect, useful for note-based applications
C RCpoll | A class for reading voltage on a digital pin, derived from http://arduino.cc/en/Tutorial/RCtime
C ReverbTank | A reverb which sounds like the inside of a tin can
C RollingAverage | Calculates a running average over a specified number of the most recent readings
C RollingStat | WARNING: this class is work in progress, don't use it yet
C Sample | Sample is like Oscil, it plays a wavetable
C SampleHuffman | A sample player for samples encoded with Huffman compression
C Smooth | A simple infinite impulse response low pass filter for smoothing control or audio signals
C Stack | A simple stack, used internally for keeping track of analog input channels as they are read
C StateVariable | A State Variable filter which offers 12db resonant low, high, bandpass and notch modes
C StereoOutput | This struct encapsulates one frame of mono audio output
C WavePacket | Wavepacket synthesis, with two overlapping streams of wave packets
C WavePacketSample | A WavePacket which allows a custom table to be set as the audio source for the wavepackets (or grains)
C WaveShaper | WaveShaper maps values from its input to values in a table, which are returned as output
C WaveShaper< char > | Int8_t specialisation of WaveShaper template
C WaveShaper< int > | Int specialisation of WaveShaper template