| Mozzi version v1.1.0 sound synthesis library for Arduino |

known_16bit_timers.h
1 #ifndef known_16bit_timers_header_
2 #define known_16bit_timers_header_
3 /*
4 Part of TimerOne library, modified by Paul S. for Teensy boards.
5 TB2012 added Leonardo section.
6 */
7
8 // Wiring-S
9 //
10 #if defined(__AVR_ATmega644P__) && defined(WIRING)
11 #define TIMER1_A_PIN 5
12 #define TIMER1_B_PIN 4
13 #define TIMER1_ICP_PIN 6
14
15
16 // Teensy 2.0
17 //
18 #elif defined(__AVR_ATmega32U4__) && defined(CORE_TEENSY)
19 #define TIMER1_A_PIN 14
20 #define TIMER1_B_PIN 15
21 #define TIMER1_C_PIN 4
22 #define TIMER1_ICP_PIN 22
23 #define TIMER1_CLK_PIN 11
24 #define TIMER3_A_PIN 9
25 #define TIMER3_ICP_PIN 10
26
27
28 // Leonardo - Make sure this is after the (__AVR_ATmega32U4__) && defined(CORE_TEENSY) entry
29 #elif defined(__AVR_ATmega32U4__)
30 #define TIMER1_A_PIN 9
31 #define TIMER1_B_PIN 10
32 #define TIMER1_C_PIN 11
33
34
35 // Teensy++ 2.0
36 #elif defined(__AVR_AT90USB1286__) && defined(CORE_TEENSY)
37 #define TIMER1_A_PIN 25
38 #define TIMER1_B_PIN 26
39 #define TIMER1_C_PIN 27
40 #define TIMER1_ICP_PIN 4
41 #define TIMER1_CLK_PIN 6
42 #define TIMER3_A_PIN 16
43 #define TIMER3_B_PIN 15
44 #define TIMER3_C_PIN 14
45 #define TIMER3_ICP_PIN 17
46 #define TIMER3_CLK_PIN 13
47
48
49 // Arduino Mega
50 //
51 #elif defined(__AVR_ATmega1280__) || defined(__AVR_ATmega2560__)
52 #define TIMER1_A_PIN 11
53 #define TIMER1_B_PIN 12
54 #define TIMER1_C_PIN 13
55 #define TIMER3_A_PIN 5
56 #define TIMER3_B_PIN 2
57 #define TIMER3_C_PIN 3
58 #define TIMER4_A_PIN 6
59 #define TIMER4_B_PIN 7
60 #define TIMER4_C_PIN 8
61 #define TIMER4_ICP_PIN 49
62 #define TIMER5_A_PIN 46
63 #define TIMER5_B_PIN 45
64 #define TIMER5_C_PIN 44
65 #define TIMER3_ICP_PIN 48
66 #define TIMER3_CLK_PIN 47
67
68
69 // Arduino Uno, Duemilanove, LilyPad, etc
70 //
71 #elif defined (__AVR_ATmega168__) || defined (__AVR_ATmega328P__)
72 #define TIMER1_A_PIN 9
73 #define TIMER1_B_PIN 10
74 #define TIMER1_ICP_PIN 8
75 #define TIMER1_CLK_PIN 5
76
77
78 // Sanguino
79 //
80 #elif defined(__AVR_ATmega644P__) || defined(__AVR_ATmega644__)
81 #define TIMER1_A_PIN 13
82 #define TIMER1_B_PIN 12
83 #define TIMER1_ICP_PIN 14
84 #define TIMER1_CLK_PIN 1
85
86 #endif
87
88 #endif