## Muse Developer Resources | Search this site

### MusePlayer
Overview MusePlayer is a utility for recording, replaying, rerouting, and converting EEG and accelerometer data from Interaxon Muse EEG devices. It can save to and convert between the native Muse datatype (.muse), Matlab (HDF5), CSV, and OSC replay formats. It is an open source project. All the source code and examples are available on Bitbucket. Currently muse-player supports the following inputs and outputs: Supported inputs: OSC network stream OSC-replay file format Muse file format v1 Muse file format v2 Supported outputs: MATLAB (click here for a description of the output) CSV OSC network stream OSC-replay file format Muse file format v2 Print to screen ## How to run it Simply type "muse-player" followed by your desired input and output arguments. See below for a description of these arguments. You can also view this information by running muse-player with no arguments - it will be printed to your screen. `optional arguments:` `` `-h, --help``` `show this help message and exit` `` `-v, --verbose` `` `Print status messages to stdout` `` `-q, --as-fast-as-possible` `` `Replay input as fast as possible instead of using` `` `original timing.` `` `-j, --jump-data-gaps``` `Replay input by omitting any data gaps larger than 1` `` `second.` `` `-n, --no--time--data``` `Replay input by omitting output of current timing` `` `info.` `` `-i FILTER_DATA [FILTER_DATA ...], --filter FILTER_DATA [FILTER_DATA ...]` `` `Filter data by path. e.g. -i /muse/dsp/elements/alpha` `` `/muse/eeg` `Input options:` `` `Only one type of input can be specified, but can be multiple files of the same type:` `` `-l [INPUT_OSC_PORT], --input-osc-port [INPUT_OSC_PORT]` `` `Listen for OSC messages on this port (default:` `` `tcp:5000).` `` `-f INPUT_MUSE_FILES [INPUT_MUSE_FILES ...], --input-muse-files INPUT_MUSE_FILES [INPUT_MUSE_FILES ...]` `` `Input from Muse file format.` `` `-o INPUT_OSCREPLAY_FILES [INPUT_OSCREPLAY_FILES ...], --input-oscreplay-files INPUT_OSCREPLAY_FILES [INPUT_OSCREPLAY_FILES ...]` `` `Input from OSC-replay files.` `Output options:` `` `One or more outputs can be specified:` `` `-s [OUTPUT_OSC_URL], --output-osc-url [OUTPUT_OSC_URL]` `` `Output OSC messages to HOST:PORT (default:` `` `osc.tcp://localhost:5000)` `` `-F FILE, --output-muse-file FILE` `` `Output to a Muse file` `` `-M FILE, --output-matlab-file FILE` `` `Output to a Matlab file` `` `-O FILE, --output-oscreplay-file FILE` `` `Output to an OSC-replay file` `` `-C FILE, --output-csv-file FILE` `` `Output to an CSV file` `` `-D, --output-screen-dump` `` `Output to the screen directly` `Examples:` `` `muse-player -f my_eeg_recording.muse -s osc.tcp://localhost:7887` `` `This will read in the file "my_eeg_recording.muse" and send those messages as OSC to port 7887.` `` `muse-player -l 5555 -M matlab.mat -s 5000` `` `This will receive OSC messages on port 5555, save them to file, and rebroadcast them to port 5000.` `` `` ``
Subpages (1): MATLAB Output File Comments